# Network UPS Tools: variable and command descriptions
#
# This file is optional.  You may delete it to save resources, but
# clients will receive "Unavailable" for any description requests.
#
# *** NOTE *** : When updating this file, also update docs/nut-names.txt

VARDESC ups.alarm "UPS alarms"
VARDESC ups.status "UPS status"
VARDESC ups.time "Internal UPS clock time"
VARDESC ups.date "Internal UPS clock date"
VARDESC ups.efficiency "Efficiency of the UPS"
VARDESC ups.model "UPS model"
VARDESC ups.mfr "UPS manufacturer"
VARDESC ups.mfr.date "UPS manufacturing date"
VARDESC ups.serial "UPS serial number"
VARDESC ups.vendorid "Vendor ID for USB devices"
VARDESC ups.productid "Product ID for USB devices"
VARDESC ups.firmware "UPS firmware"
VARDESC ups.firmware.aux "Auxiliary device firmware"
VARDESC ups.temperature "UPS temperature (degrees C)"
VARDESC ups.load "Load on UPS (percent of full)"
VARDESC ups.load.energysave "Load on UPS that triggers energysave (percent)"
VARDESC ups.load.high "Load when UPS switches to overload condition (percent)"
VARDESC ups.id "UPS system identifier"
VARDESC ups.delay.start "Interval to wait before (re)starting the load (seconds)"
VARDESC ups.delay.reboot "Interval to wait before rebooting the UPS (seconds)"
VARDESC ups.delay.shutdown "Interval to wait after shutdown with delay command (seconds)"
VARDESC ups.timer.start "Time before the load will be started (seconds)"
VARDESC ups.timer.reboot "Time before the load will be rebooted (seconds)"
VARDESC ups.timer.shutdown "Time before the load will be shutdown (seconds)"
VARDESC ups.test.interval "Interval between self tests (seconds)"
VARDESC ups.test.result "Results of last self test"
VARDESC ups.display.language "Language to use on front panel"
VARDESC ups.contacts "UPS external contact sensors"
VARDESC ups.power "Current value of apparent power (VA)"
VARDESC ups.power.nominal "UPS power rating (VA)"
VARDESC ups.realpower "Current value of real power (W)"
VARDESC ups.realpower.nominal "UPS real power rating (W)"
VARDESC ups.beeper.status "UPS beeper status"
VARDESC ups.type "UPS type"
VARDESC ups.start.auto "UPS starts when mains is (re)applied"
VARDESC ups.start.battery "Allow to start UPS from battery"
VARDESC ups.start.reboot "UPS reboots when power returns during shutdown delay"
VARDESC ups.shutdown "Enable or disable UPS shutdown ability (poweroff)"

VARDESC input.voltage "Input voltage (V)"
VARDESC input.voltage.extended "Extended input voltage range"
VARDESC input.voltage.maximum "Maximum incoming voltage seen (V)"
VARDESC input.voltage.minimum "Minimum incoming voltage seen (V)"
VARDESC input.voltage.status "Voltage status relative to the thresholds"
VARDESC input.voltage.low.warning "Input voltage low warning threshold (V)"
VARDESC input.voltage.low.critical "Input voltage low critical threshold (V)"
VARDESC input.voltage.high.warning "Input voltage high warning threshold (V)"
VARDESC input.voltage.high.critical "Input voltage high critical threshold (V)"
VARDESC input.voltage.nominal "Nominal input voltage (V)"
VARDESC input.transfer.reason "Reason for last transfer to battery"
VARDESC input.transfer.low "Low voltage transfer point (V)"
VARDESC input.transfer.high "High voltage transfer point (V)"
VARDESC input.transfer.eco.low "Low voltage ECO transfer point (V)"
VARDESC input.transfer.bypass.low "Low voltage Bypass transfer point (V)"
VARDESC input.transfer.eco.high "High voltage ECO transfer point (V)"
VARDESC input.transfer.bypass.high "High voltage Bypass transfer point (V)"
VARDESC input.transfer.frequency.bypass.range "Frequency range Bypass transfer point (percent of nominal Hz)"
VARDESC input.transfer.frequency.eco.range "Frequency range ECO transfer point (percent of nominal Hz)"
VARDESC input.transfer.hysteresis "Threshold of switching protection modes, voltage transfer point (V)"
VARDESC input.transfer.low.min "smallest settable low voltage transfer point (V)"
VARDESC input.transfer.low.max "greatest settable low voltage transfer point (V)"
VARDESC input.transfer.high.min "smallest settable high voltage transfer point (V)"
VARDESC input.transfer.high.max "greatest settable high voltage transfer point (V)"
VARDESC input.eco.switchable "Input High Efficiency (aka ECO) mode switch"
VARDESC input.transfer.bypass.forced "Rule for allow auto Bypass switch (on/off) transfer modes (enabled or disabled)"
VARDESC input.transfer.bypass.overload "Rule for auto transfer on Bypass when overload (enabled or disabled)"
VARDESC input.transfer.bypass.outlimits "Rule for auto transfer on Bypass when out of tolerance (enabled or disabled)"
VARDESC input.bypass.switchable "Input auto transfer on Bypass when overload or out of tolerance (enabled or disabled)"
VARDESC input.bypass.switch.on "Put the UPS in Bypass mode"
VARDESC input.bypass.switch.off "Take the UPS out of Bypass mode"
VARDESC input.bypass.voltage "Input bypass voltage (V)"
VARDESC input.bypass.frequency "Input bypass frequency (Hz)"
VARDESC input.sensitivity "Input power sensitivity"
VARDESC input.quality "Input power quality"
VARDESC input.current "Input current (A)"
VARDESC input.current.nominal "Nominal input current (A)"
VARDESC input.current.status "Current status relative to the thresholds"
VARDESC input.current.low.warning "Input current low warning threshold (A)"
VARDESC input.current.low.critical "Input current low critical threshold (A)"
VARDESC input.current.high.warning "Input current high warning threshold (A)"
VARDESC input.current.high.critical "Input current high critical threshold (A)"
VARDESC input.frequency "Input line frequency (Hz)"
VARDESC input.frequency.extended "Extended input frequency range"
VARDESC input.frequency.status "Frequency status"
VARDESC input.frequency.nominal "Nominal input line frequency (Hz)"
VARDESC input.frequency.low "Minimum input line frequency (Hz)"
VARDESC input.frequency.high "Maximum input line frequency (Hz)"
VARDESC input.transfer.boost.low "Low voltage boosting transfer point (V)"
VARDESC input.transfer.boost.high "High voltage boosting transfer point (V)"
VARDESC input.transfer.trim.low "Low voltage trimming transfer point (V)"
VARDESC input.transfer.trim.high "High voltage trimming transfer point (V)"
VARDESC input.transfer.delay "Delay before transfer to mains"
VARDESC input.load "Load on (ePDU) input (percent of full)"
VARDESC input.realpower "Current sum value of all (ePDU) phases real power (W)"
VARDESC input.power "Current sum value of all (ePDU) phases apparent power (VA)"
VARDESC input.source "The current input power source"
VARDESC input.source.preferred "The preferred input power source"

VARDESC output.voltage "Output voltage (V)"
VARDESC output.voltage.nominal "Nominal output voltage (V)"
VARDESC output.frequency "Output frequency (Hz)"
VARDESC output.frequency.nominal "Nominal output frequency (Hz)"
VARDESC output.current "Output current (A)"
VARDESC output.current.nominal "Nominal output current (A)"

VARDESC battery.charge "Battery charge (percent of full)"
VARDESC battery.charge.approx "Rough approximation of battery charge"
VARDESC battery.charge.low "Remaining battery level when UPS switches to LB (percent)"
VARDESC battery.charge.restart "Minimum battery level for restart after power off (percent)"
VARDESC battery.charge.warning "Battery level when UPS switches to Warning state (percent)"
VARDESC battery.voltage "Battery voltage (V)"
VARDESC battery.current "Battery current (A)"
VARDESC battery.capacity "Battery capacity (Ah)"
VARDESC battery.temperature "Battery temperature (degrees C)"
VARDESC battery.voltage.nominal "Nominal battery voltage (V)"
VARDESC battery.runtime "Battery runtime (seconds)"
VARDESC battery.runtime.low "Remaining battery runtime when UPS switches to LB (seconds)"
VARDESC battery.alarm.threshold "Battery alarm threshold"
VARDESC battery.date "Battery change date"
VARDESC battery.mfr.date "Battery manufacturing date"
VARDESC battery.packs "Number of battery packs"
VARDESC battery.packs.bad "Number of bad battery packs"
VARDESC battery.type "Battery chemistry"
VARDESC battery.protection "Prevent deep discharge of battery"
VARDESC battery.energysave "Switch off when running on battery and no/low load"
VARDESC battery.energysave.load "Switch off UPS if on battery and load level lower (percent)"
VARDESC battery.energysave.delay "Delay before switch off UPS if on battery and load level low (min)"
VARDESC battery.energysave.realpower "Switch off UPS if on battery and load level lower (Watts)"
VARDESC battery.charger.status "Battery charger status"
VARDESC battery.charger.type "Type of battery charger"

VARDESC ambient.temperature "Ambient temperature (degrees C)"
VARDESC ambient.temperature.alarm "Ambient temperature alarm is active"
VARDESC ambient.temperature.status "Ambient temperature status relative to the configured thresholds"
VARDESC ambient.temperature.alarm.maximum "Maximum allowed ambient temperature (degrees C)"
VARDESC ambient.temperature.alarm.minimum "Minimum allowed ambient temperature (degrees C)"
VARDESC ambient.temperature.alarm.enable "Enable ambient temperature alarm"
VARDESC ambient.temperature.low "Temperature threshold low (degrees C)"
VARDESC ambient.temperature.low.warning "Temperature threshold low warning (degrees C)"
VARDESC ambient.temperature.low.critical "Temperature threshold low critical (degrees C)"
VARDESC ambient.temperature.high "Temperature threshold high (degrees C)"
VARDESC ambient.temperature.high.warning "Temperature threshold high warning (degrees C)"
VARDESC ambient.temperature.high.critical "Temperature threshold high critical (degrees C)"
VARDESC ambient.humidity "Ambient humidity (percent)"
VARDESC ambient.humidity.alarm "Ambient humidity alarm is active"
VARDESC ambient.humidity.status "Ambient humidity status relative to the configured thresholds"
VARDESC ambient.humidity.alarm.maximum "Maximum allowed ambient humidity (percent)"
VARDESC ambient.humidity.alarm.minimum "Minimum allowed ambient humidity (percent)"
VARDESC ambient.humidity.alarm.enable "Enable ambient humidity alarm"
VARDESC ambient.humidity.low "Ambient humidity threshold low (percent)"
VARDESC ambient.humidity.low.warning "Ambient humidity threshold low warning (percent)"
VARDESC ambient.humidity.low.critical "Ambient humidity threshold low critical (percent)"
VARDESC ambient.humidity.high "Ambient humidity threshold high (percent)"
VARDESC ambient.humidity.high.warning "Ambient humidity threshold high warning (percent)"
VARDESC ambient.humidity.high.critical "Ambient humidity threshold high critical (percent)"
VARDESC ambient.present "Ambient sensor presence"
VARDESC ambient.contacts.1.status "State of the dry contact sensor 1"
VARDESC ambient.contacts.2.status "State of the dry contact sensor 2"

# FIXME: the outlet collection is indexed - solve with regexps?
#
# VARDESC outlet.[[:digit:]]+.id "Outlet system identifier (<index>)"

VARDESC outlet.id "Outlet system identifier"
VARDESC outlet.desc "Outlet description"
VARDESC outlet.switch "Outlet switch control"
VARDESC outlet.status "Outlet switch status"
VARDESC outlet.protect.status "Outlet protection status"
VARDESC outlet.switchable "Outlet switch ability"
VARDESC outlet.autoswitch.charge.low "Remaining battery level to power off this outlet (percent)"
VARDESC outlet.delay.shutdown "Interval to wait before shutting down this outlet (seconds)"
VARDESC outlet.delay.start "Interval to wait before restarting this outlet (seconds)"
VARDESC outlet.1.id "Outlet system identifier"
VARDESC outlet.1.desc "Outlet description"
VARDESC outlet.1.switch "Outlet switch control"
VARDESC outlet.1.status "Outlet switch status"
VARDESC outlet.1.protect.status "Outlet protection status"
VARDESC outlet.1.switchable "Outlet switch ability"
VARDESC outlet.1.ecocontrol "Master Outlet used to automatically power off the slave outlets"
VARDESC outlet.1.autoswitch.charge.low "Remaining battery level to power off this outlet (percent)"
VARDESC outlet.1.delay.shutdown "Interval to wait before shutting down this outlet (seconds)"
VARDESC outlet.1.delay.start "Interval to wait before restarting this outlet (seconds)"
VARDESC outlet.1.designator "Outlet designator"
VARDESC outlet.2.id "Outlet system identifier"
VARDESC outlet.2.desc "Outlet description"
VARDESC outlet.2.switch "Outlet switch control"
VARDESC outlet.2.status "Outlet switch status"
VARDESC outlet.2.protect.status "Outlet protection status"
VARDESC outlet.2.switchable "Outlet switch ability"
VARDESC outlet.2.ecocontrol "Master Outlet used to automatically power off the slave outlets"
VARDESC outlet.2.autoswitch.charge.low "Remaining battery level to power off this outlet (percent)"
VARDESC outlet.2.delay.shutdown "Interval to wait before shutting down this outlet (seconds)"
VARDESC outlet.2.delay.start "Interval to wait before restarting this outlet (seconds)"

VARDESC device.part "Device part number"
VARDESC device.mfr "Device manufacturer"
VARDESC device.model "Device model"
VARDESC device.serial "Device serial number"
VARDESC device.type "Device type"
VARDESC device.description "Device description"
VARDESC device.contact "Device administrator name"
VARDESC device.location "Device physical location"
VARDESC device.macaddr "Physical network address of the device"
VARDESC device.uptime "Device uptime in seconds"
VARDESC device.count "Total number of daisychained devices"
VARDESC device.usb.version "Device USB version"

VARDESC server.info "Server information"
VARDESC server.version "Server version"

VARDESC driver.name "Driver name"
VARDESC driver.debug "Current debug verbosity level of the driver program"
# Note: normally a `drivername -k` call is used during shutdowns,
# and at that time the daemon instance of the driver must be stopped:
VARDESC driver.flag.allow_killpower "Safety flip-switch to allow the driver daemon to send UPS shutdown command (accessible via driver.killpower)"
VARDESC driver.version "Driver version - NUT release"
VARDESC driver.version.internal "Internal driver version"
VARDESC driver.version.usb "USB library version"
VARDESC driver.version.data "Version of the internal data mapping, for generic drivers"
VARDESC driver.state "Current state in driver's lifecycle"

# FIXME: driver.parameter and driver.flag can have many possible members
#
# VARDESC driver.parameter.[[:alpha:]]+ "Driver parameter: <name>"
# VARDESC driver.flag.[[:alpha:]]+ "Driver flag: <name>"

CMDDESC driver.exit "Tell the driver daemon to just exit its program (so the caller or service management framework can restart it with new options)"
CMDDESC driver.killpower "Tell the driver daemon to initiate UPS shutdown; should be unlocked with driver.flag.allow_killpower option or variable setting"
CMDDESC driver.reload "Reload running driver configuration from the file system (only works for changes in some options)"
CMDDESC driver.reload-or-error "Reload running driver configuration from the file system (only works for changes in some options); return an error if something changed and could not be applied live (so the caller can restart it with new options)"
CMDDESC driver.reload-or-exit "Reload running driver configuration from the file system (only works for changes in some options); exit the running driver if something changed and could not be applied live (so service management framework can restart it with new options)"

CMDDESC load.off "Turn off the load immediately"
CMDDESC load.on "Turn on the load immediately"
CMDDESC shutdown.default "Run the driver-defined UPS shutdown sequence (as opposed to user-configured 'sdcommands')"
CMDDESC shutdown.return "Turn off the load and return when power is back"
CMDDESC shutdown.stayoff "Turn off the load and remain off"
CMDDESC shutdown.stop "Stop a shutdown in progress"
CMDDESC shutdown.reboot "Shut down the load briefly while rebooting the UPS"
CMDDESC shutdown.reboot.graceful "Delay briefly then shut down the load while rebooting the UPS"
CMDDESC test.panel.start "Start testing the UPS panel"
CMDDESC test.panel.stop "Stop a UPS panel test"
CMDDESC test.failure.start "Start a simulated power failure"
CMDDESC test.failure.stop "Stop simulating a power failure"
CMDDESC test.battery.start "Start a battery test"
CMDDESC test.battery.start.quick "Start a quick battery test"
CMDDESC test.battery.start.deep "Start a deep battery test"
CMDDESC test.battery.stop "Stop the battery test"
CMDDESC test.system.start "Start a system test"
CMDDESC calibrate.start "Start run time calibration"
CMDDESC calibrate.stop "Stop run time calibration"
CMDDESC bypass.start "Put the UPS in Bypass mode"
CMDDESC bypass.stop "Take the UPS out of Bypass mode"
CMDDESC experimental.ecomode.start "Put UPS in High Efficiency (aka ECO) mode"
CMDDESC experimental.ecomode.stop "Take the UPS out of High Efficiency (aka ECO) mode"
CMDDESC experimental.bypass.ecomode.start "Put UPS in Bypass mode then High Efficiency (aka ECO) mode"
CMDDESC experimental.bypass.ecomode.stop "Take the UPS out of High Efficiency (aka ECO) mode after exiting Bypass mode"
CMDDESC experimental.essmode.start "Put UPS in Energy Saver System (aka ESS) mode"
CMDDESC experimental.essmode.stop "Take the UPS out of Energy Saver System (aka ESS) mode"
CMDDESC experimental.test.beeper.start "Start testing the UPS beeper"
CMDDESC experimental.test.beeper.stop "Stop a UPS beeper test"
CMDDESC reset.input.minmax "Reset minimum and maximum input voltage status"
CMDDESC reset.watchdog "Reset watchdog timer"
CMDDESC beeper.on "Obsolete (use beeper.enable)"
CMDDESC beeper.off "Obsolete (use beeper.disable or beeper.mute)"
CMDDESC beeper.enable "Enable the UPS beeper"
CMDDESC beeper.disable "Disable the UPS beeper"
CMDDESC beeper.mute "Temporarily mute the UPS beeper"
CMDDESC beeper.toggle "Toggle the UPS beeper"
CMDDESC outlet.1.load.off "Turn off the load on outlet 1 immediately"
CMDDESC outlet.1.load.on "Turn on the load on outlet 1 immediately"
CMDDESC outlet.1.shutdown.return "Turn off the outlet 1 and return when power is back"
CMDDESC outlet.2.load.off "Turn off the load on outlet 2 immediately"
CMDDESC outlet.2.load.on "Turn on the load on outlet 2 immediately"
CMDDESC outlet.2.shutdown.return "Turn off the outlet 2 and return when power is back"

# The following two commands should *only* be defined when you need
# to compose a 'shutdown.return' command by sending both a switch-off
# with delay and a switch-on with delay command to the UPS. If this
# can be done with a single command, use 'shutdown.return' instead.
# Note that the switch-on with delay command *must not* turn on the
# load if the UPS is on battery.
#
CMDDESC load.off.delay "Turn off the load with a delay (seconds)"
CMDDESC load.on.delay "Turn on the load with a delay (seconds)"
